Jitter Buffer

A jitter buffer is storage for voice packets so they can be sent out in evenly spaced intervals used to reduce jitter, providing better transmission reliability.

There are two jitter buffer implementation types which are used by the SIP channel reciever.

Implementation	Description
Fixed	Use a fixed buffer size.
Adaptive	Use a variable buffer size.