802.11ac

802.11ac is a wireless radio specification for both the 2.4 GHz and the 5 GHz bands with support for multiple-input multiple-output antennas, providing a maximum data rate from 433 Mbit/s to 1300 Mbit/s.