STUN

Session Traversal Utilities for NAT (STUN) consists of methods and a protocol to allow a server to discover its public IP address from behind a NAT. It is used for real-time voice, video, messaging, and other interactive IP services.

The protocol requires a STUN server located on the public side of the NAT.